# ExternalAntenna

Antenna for LTE or radio communication

| **Key features** | **Communication channels**  2G/3G/LTE  Jeweller  Wings  **Operating frequencies**  698–960 MHz  1,710–2,690 MHz  **Connector**  SMA |
| --- | --- |
| **Sabotage protection** | **External antenna breakage detection**  An Ajax system is able to detect a breakage of an external antenna and notify users and the monitoring company. |
| **Installation** | * The antenna is connected to the hub’s communication channels and goes outside through holes in the hub’s casing. * The antenna is attached to the surface using a pre-applied double-sided adhesive tape. |
| **Enclosure** | **Dimensions**  115.6 × 21.7 × 5.8 mm  4.55″ × 0.85″ × 0.23″  **Cable length**  3,000 mm  9.84″  **Weight**  41 g  1.45 oz  **Operating temperature range**  from –40 °C to +85 °C  from –40 °F to 185 °F  **Operating humidity**  up to 95% |
| **Colors** | Black |
| **Complete set** | ExternalAntenna  Quick start guide |
| **Warranty** | 24 months |