# ExternalAntenna

Antenna for LTE or radio communication

| **Key features** | **Communication channels**2G/3G/LTE JewellerWings**Operating frequencies**698–960 MHz1,710–2,690 MHz**Connector**SMA |
| --- | --- |
| **Sabotage protection** | **External antenna breakage detection**An Ajax system is able to detect a breakage of an external antenna and notify users and the monitoring company. |
| **Installation** | * The antenna is connected to the hub’s communication channels and goes outside through holes in the hub’s casing.
* The antenna is attached to the surface using a pre-applied double-sided adhesive tape.
 |
| **Enclosure** | **Dimensions**115.6 × 21.7 × 5.8 mm4.55″ × 0.85″ × 0.23″**Cable length**3,000 mm9.84″**Weight**41 g1.45 oz**Operating temperature range**from –40 °C to +85 °Cfrom –40 °F to 185 °F**Operating humidity**up to 95% |
| **Colors** | Black |
| **Complete set** | ExternalAntennaQuick start guide |
| **Warranty** | 24 months |