## BulletCam

Wired IP camera

| **Compatibility** | **Control panels**  Hub  Hub Plus  Hub 2 (2G)  Hub 2 (4G)  Hub 2 Plus  Hub Hybrid (2G)  Hub Hybrid (4G)  **Video recorders**  NVR |
| --- | --- |
| **Models** | **5 MP/2.8 mm**   * Resolution up to 2880 × 1620 px * Frame rate up to 25 FPS * Viewing angle from 100° to 110°   **5 MP/4 mm**   * Resolution up to 2880 × 1620 px * Frame rate up to 25 FPS * Viewing angle from 75° to 85°   **8 MP/2.8 mm**   * Resolution up to 3840 × 2160 px * Frame rate up to 20 FPS * Viewing angle from 100° to 110°   **8 MP/4 mm**   * Resolution up to 3840 × 2160 px * Frame rate up to 20 FPS * Viewing angle from 75° to 85° |
| **Videostream** | **Video protocol**  JetSparrow  Fast and encrypted peer-to-peer video protocol developed by Ajax Systems.  **Storage**  **NVR**  Hard drive with a capacity of up to 16 TB (SATA connectivity, 3.5” size). Memory storage device not included.  **microSD**  Up to 256 GB. Memory storage device not included.  **Video codec**  H.265  H.264  **Dynamic range**  True WDR |
| **Communication channel** | **Ethernet**  up to 100 Mbps |
| **Key features** | **Motion detection**  The camera has software to detect motion in the frame.  **Object detection**  using AI   * Humans. * Pets. * Vehicles.   **Smart IR illumination**  up to 35 m  Automatic adjustment of intensity in real time to avoid overexposure. This allows you to see objects that are far away or too close to the camera in low light conditions.  **Visual verification of Ajax alarms**  The system allows you to set up a scenario when Ajax detectors activate selected cameras to start recording. The result is immediately sent to the mobile or desktop monitoring app.  **Microphone**  With the corresponding settings, the camera records sound at the object.  **Audio codec**  G711-ULAW  G711-ALAW  G726  G722 |
| **Power supply** | **Power supply unit**  12 V⎓ ± 20%, 1 А  Up to 15 W of mains power consumption.  **Ethernet port**  PoE Standard 802.3at |
| **Sabotage protection** | **mTLS**  Encrypted connection for data protection.  **Authentication**  via Cloud  Without local access rights.  **Secure Boot**  Protection against firmware spoofing.  **OTA signature verification**  Secure automatic firmware update.  **Privacy**  Access rights distribution for users in mobile apps and for monitoring operators in PRO Desktop. |
| **Enclosure** | **Dimensions**  198 × 76 × 76 mm  7.8″ × 2.99″ × 2.99″  **Weight**  550 g  19.4 oz  **Operating temperature range**  from −30 °C to +60 °C  from −22 °F to 140 °F  **Operating humidity**  up to 90%  **Protection class**  IP65 |
| **Colours** | **Black**  **White** |
| **Complete set** | BulletCam  Installation template  Installation kit  Quick start guide |
| **Warranty** | 24 months |