# Internal battery NB (7.2V/95Ah)

Pack of 10 LTC ER34615-LD non-rechargeable batteries to install into Hub BP Jeweller

| **Battery type** | **Batteries**  10 × ER34615  Non-rechargeable, lithium thionyl chloride battery with HPC-1520 pulse capacitor.  **Nominal voltage**  7.2 V⎓  **Capacity**  95 Ah |
| --- | --- |
| **Power supply** | **Maximum load current**  700 mA  **End-of-life battery voltage**  4 V⎓ |
| **Recommendations** | Do not short the power terminals.  Do not recharge the battery.  Use the battery with compatible devices only.  The battery is designed for indoor use only. |
| **Enclosure** | **Dimensions**  135 × 65 × 105 mm  5.31" × 2.56" × 4.13"  **Weight**  990 g  35 oz  **Battery connector type**  Molex 2139-2  **Operating temperature range**  from −10 °C to +40 °C  from 14 °F to 104 °F  **Operating humidity**  up to 75% |
| **Complete set** | Internal battery NB (7.2V/95Ah) |
| **Warranty** | 24 months |