# Internal battery NB (7.2V/95Ah)

Pack of 10 LTC ER34615-LD non-rechargeable batteries to install into Hub BP Jeweller

| **Battery type** | **Batteries**10 × ER34615Non-rechargeable, lithium thionyl chloride battery with HPC-1520 pulse capacitor.**Nominal voltage**7.2 V⎓**Capacity**95 Ah |
| --- | --- |
| **Power supply** | **Maximum load current**700 mA**End-of-life battery voltage**4 V⎓ |
| **Recommendations** | Do not short the power terminals.Do not recharge the battery.Use the battery with compatible devices only.The battery is designed for indoor use only. |
| **Enclosure** | **Dimensions**135 × 65 × 105 mm5.31" × 2.56" × 4.13"**Weight**990 g35 oz**Battery connector type**Molex 2139-2**Operating temperature range**from −10 °C to +40 °Cfrom 14 °F to 104 °F**Operating humidity**up to 75% |
| **Complete set** | Internal battery NB (7.2V/95Ah) |
| **Warranty** | 24 months |