# SurfaceBox [55]

Surface mounting box for one LightSwitch or Outlet device

| **Compatibility** | **LightSwitch devices**LightSwitch (1-gang) JewellerLightSwitch (2-gang) JewellerLightSwitch (2-way) JewellerLightSwitch (2-gang/2-way) JewellerLightSwitch (Crossover) JewellerLightSwitch (Dimmer) Jeweller**Outlet devices**Outlet [type E] JewellerOutlet [type F] JewellerOutlet (basic) [type E]Outlet (basic) [type F] |
| --- | --- |
| **Colors** | **White****RAL 9003** |
| **Key features** | **Color and shape matching**The SurfaceBox [55] shape smoothly aligns with the LightSwitch touch-sensitive panel and Outlet cover.**Easy installation**Various fixing points to mount SurfaceBox [55] on any surface.**Cable routing**Dedicated spots to route the wires in SurfaceBox [55] from the back or side.**Form factor of the LightSwitch or Outlet device**European type (55) |
| **Recommendations** | The device is designed for indoor use only. A professional electrician should install the device. |
| **Enclosure** | **Dimensions**82.6 × 82.6 × 46.8 mm3.25" × 3.25" × 1.84"**Weight**63.5 g2.24 oz**Material**polycarbonate**Operating temperature range**from –10 °C to +40 °Cfrom 14 °F to 104 °F**Operating humidity**up to 75% with no condensation**Protection class**IP20 |
| **Complete set** | SurfaceBox [55]4 screws for LightSwitch or Outlet device mountingQuick start guide |
| **Warranty** | 24 months |