# SurfaceBox [55]

Surface mounting box for one LightSwitch or Outlet device

| **Compatibility** | **LightSwitch devices**  LightSwitch (1-gang) Jeweller  LightSwitch (2-gang) Jeweller  LightSwitch (2-way) Jeweller  LightSwitch (2-gang/2-way) Jeweller  LightSwitch (Crossover) Jeweller  LightSwitch (Dimmer) Jeweller  **Outlet devices**  Outlet [type E] Jeweller  Outlet [type F] Jeweller  Outlet (basic) [type E]  Outlet (basic) [type F] |
| --- | --- |
| **Colors** | **White**  **RAL 9003** |
| **Key features** | **Color and shape matching**  The SurfaceBox [55] shape smoothly aligns with the LightSwitch touch-sensitive panel and Outlet cover.  **Easy installation**  Various fixing points to mount SurfaceBox [55] on any surface.  **Cable routing**  Dedicated spots to route the wires in SurfaceBox [55] from the back or side.  **Form factor of the LightSwitch or Outlet device**  European type (55) |
| **Recommendations** | The device is designed for indoor use only. A professional electrician should install the device. |
| **Enclosure** | **Dimensions**  82.6 × 82.6 × 46.8 mm  3.25" × 3.25" × 1.84"  **Weight**  63.5 g  2.24 oz  **Material**  polycarbonate  **Operating temperature range**  from –10 °C to +40 °C  from 14 °F to 104 °F  **Operating humidity**  up to 75% with no condensation  **Protection class**  IP20 |
| **Complete set** | SurfaceBox [55]  4 screws for LightSwitch or Outlet device mounting  Quick start guide |
| **Warranty** | 24 months |