## NVR

Network video recorder

| **Compatibility** | **Compatible hub models**HubHub PlusHub 2 (2G)Hub 2 (4G)Hub 2 PlusHub Hybrid (2G)Hub Hybrid (4G) |
| --- | --- |
| **Videostream** | **NVR models**8-channel16-channelWith up to 4K resolution (25/30 FPS).**IP cameras*** ONVIF (Profile S/T)
* RTSP

**Storage**hard drive with a capacity of up to 16 TB (SATA connectivity, 3.5” size)HDD not included.**Decoding formats**H.265H.264**Bandwidth**up to 100 Mbps |
| **Recommendations** | The device operating voltage is 110–240 V~.NVR is designed for indoor installation only. |
| **Communication channels** | **Ethernet**up to 100 Mbps**Bluetooth**BLE frequency band: 2.400–2.4835 GHzTo set up an Ethernet connection.**Radio signal power**2.5 mW (100 mW limit) |
| **Key features** | **Motion detection**NVR has built-in software to detect the motion in the frame. Possible to switch between image analysis by NVR or camera algorithms.**In-app video management system*** Videowall that combines images from all connected cameras.
* Event filters.
* Timeline with smooth preview.

**Visual verification of Ajax alarms**NVR allows setting up a scenario in which Ajax detectors trigger specific cameras to start recording. This results straight in mobile and desktop (monitoring) apps.**Privacy**Access rights distribution for users in mobile apps and for monitoring operators in PRO Desktop. |
| **Power supply** | **Main** 110–240 V~, 50/60 Hz, 0.6 AUp to 24 W of mains power consumption.**Backup** CR2032 battery, 3 VOnly to power the system clock. |
| **Anti-sabotage** | **Tamper alarm**Notifications about attempts to detach the device from the surface or remove it from the mounting panel. |
| **Enclosure** | **Dimensions**251 × 251 × 51 mm**/**9.88″ × 9.88″ × 2.01″**Weight**700 g/24.69 ozWithout a hard drive.**Operating temperature range**from 0°C to +40°C**/**from 32°F to 104°F**Operating humidity**up to 75%**Protection class**IP20 |
| **Colours** | **Black****White** |
| **Complete set** | NVRSmartBracket mounting panelPower cableEthernet cableInstallation kitQuick Start Guide |
| **Warranty** | 24 months |