## NVR

Network video recorder

| **Compatibility** | **Compatible hub models**  Hub  Hub Plus  Hub 2 (2G)  Hub 2 (4G)  Hub 2 Plus  Hub Hybrid (2G)  Hub Hybrid (4G) |
| --- | --- |
| **Videostream** | **NVR models**  8-channel  16-channel  With up to 4K resolution (25/30 FPS).  **IP cameras**   * ONVIF (Profile S/T) * RTSP   **Storage**  hard drive with a capacity of up to 16 TB (SATA connectivity, 3.5” size)  HDD not included.  **Decoding formats**  H.265  H.264  **Bandwidth**  up to 100 Mbps |
| **Recommendations** | The device operating voltage is 110–240 V~.  NVR is designed for indoor installation only. |
| **Communication channels** | **Ethernet**  up to 100 Mbps  **Bluetooth**  BLE frequency band: 2.400–2.4835 GHz  To set up an Ethernet connection.  **Radio signal power**  2.5 mW (100 mW limit) |
| **Key features** | **Motion detection**  NVR has built-in software to detect the motion in the frame. Possible to switch between image analysis by NVR or camera algorithms.  **In-app video management system**   * Videowall that combines images from all connected cameras. * Event filters. * Timeline with smooth preview.   **Visual verification of Ajax alarms**  NVR allows setting up a scenario in which Ajax detectors trigger specific cameras to start recording. This results straight in mobile and desktop (monitoring) apps.  **Privacy**  Access rights distribution for users in mobile apps and for monitoring operators in PRO Desktop. |
| **Power supply** | **Main**  110–240 V~, 50/60 Hz, 0.6 A  Up to 24 W of mains power consumption.  **Backup**  CR2032 battery, 3 V  Only to power the system clock. |
| **Anti-sabotage** | **Tamper alarm**  Notifications about attempts to detach the device from the surface or remove it from the mounting panel. |
| **Enclosure** | **Dimensions**  251 × 251 × 51 mm**/**9.88″ × 9.88″ × 2.01″  **Weight**  700 g/24.69 oz  Without a hard drive.  **Operating temperature range**  from 0°C to +40°C**/**from 32°F to 104°F  **Operating humidity**  up to 75%  **Protection class**  IP20 |
| **Colours** | **Black**  **White** |
| **Complete set** | NVR  SmartBracket mounting panel  Power cable  Ethernet cable  Installation kit  Quick Start Guide |
| **Warranty** | 24 months |